**Solar Energy Project 2: Modelling Radiation and Electricity Generation**

*Prepared by: [Your Names]*  
*Deadline: November 19, 2023*

**1. Introduction**

In this project, our goal was to model the electricity generated by the solar photovoltaic installation on the rooftop of the Navitas building in Aarhus and compare it with experimentally measured data to assess model accuracy. The project involved modelling hourly global radiation, estimating direct and diffuse radiation, and simulating power generation from the PV modules based on environmental parameters.

**2. Modelling Hourly Global Radiation**

We initiated the project by modelling the hourly global radiation on a horizontal surface (Gt(0)) in Aarhus throughout 2018. Figure 1 illustrates the plotted global radiation for the first weeks of February and June 2018, showcasing seasonal variations.

*[Figure 1: Hourly Global Radiation in Aarhus for February and June 2018]*

**3. Estimating Diffuse Fraction from Cloud Cover**

Using cloud cover ratios obtained from the weather station's data for 2018, we estimated the diffuse fraction (FD) as FD = Cloud cover / 100.

**4. Modelling Direct and Diffuse Radiation**

Utilizing the estimated diffuse fraction, we calculated direct and diffuse radiation on the horizontal surface in Aarhus. Figure 2 depicts the modelled global radiation on the PV module surfaces for the first weeks of February and June 2018, illustrating variations corresponding to seasonal changes.

*[Figure 2: Global Radiation on PV Module Surfaces for February and June 2018]*

**5. Estimation of Power Production from PV Modules**

We estimated the power produced by the installation at every hour, considering the irradiance at the PV module entrance and power reduction due to ambient temperature.

**6. Comparison with Measured Production**

To compare modelled generation with historical data, we plotted the measured production provided by the Facility Management at Navitas. Figure 3 presents the comparison for the first weeks of February and June 2018.

*[Figure 3: Comparison between Measured and Modelled Production for February and June 2018]*

**7. Assessment of Model Accuracy**

We conducted a relative root mean square error (RMSE) analysis between the modelled and historically measured generation on hourly, daily, weekly, and monthly scales. This analysis provided insights into model accuracy and error trends over different time periods.

**8. Conclusion**

This report summarizes our methodologies, findings, and insights gained from modelling solar radiation and electricity generation. The accompanying figures provide a visual representation of the data and comparisons made, supporting our analysis of solar energy potential at the Navitas building in Aar

1. Overview

Our objective in this research was to estimate the electricity produced by the solar photovoltaic installation on the roof of the Navitas building in Aarhus and evaluate the model's correctness by comparing it with empirically observed data. The project comprised simulating power generation from the PV modules depending on environmental conditions, modeling hourly global radiation, and estimating direct and diffuse radiation.

2. Hourly Global Radiation Modeling

In 2018, we started the experiment by simulating the hourly global radiation in Aarhus on a horizontal surface (Gt(0)). Plotted worldwide radiation for the first weeks of February and June 2018, including seasonal changes, is shown in Figure 1.

[Figure1: Aarhus, Denmark, Hourly Global Radiation for February and June 2018]

3. Utilizing Cloud Cover to Estimate Diffuse Fraction

3. Utilizing Cloud Cover to Estimate Diffuse Fraction

We calculated the diffuse fraction (FD) using cloud cover ratios from the weather station's 2018 data, which is equal to FD = Cloud cover / 100.

4. Direct and Diffuse Radiation Modeling

We computed direct and diffuse radiation on the horizontal surface in Aarhus using the expected diffuse fraction. Figure 2 shows variations in global radiation that correlate to seasonal changes on the PV module surfaces between the first weeks of February and June 2018.

[Figure 2: February and June 2018 Global Radiation on PV Module Surfaces]

5. Calculating PV Module Power Production

Taking into account the irradiance at the PV module entrance and power loss because of, we calculated the power generated by the system at each hour.

5. Calculating PV Module Power Production

Taking into account the irradiance at the PV module entrance and power loss from ambient temperature, we calculated the power generated by the installation at each hour.

6. Evaluation in Light of Measured Production

We showed the measured production provided by Navitas Facility Management to compare the modeled generation with historical data. The comparison for the first weeks of February and June 2018 is shown in Figure 3.

[Figure 3: February and June 2018 Measured and Modeled Production Comparison]

7. Evaluation of Model Precision

On hourly, daily, weekly, and monthly timescales, we performed a relative root mean square error (RMSE) comparison between the historically measured generation and the simulated generation. This investigation revealed patterns in model accuracy and error across